

***** DAS Statistics *****

   * Id: 0
   * Type: 4 LX-4000 DAS
   * Version: 6
   * Data Rate: 120
   * Sample Size: 4
   * Number of Sensors: 10
      1) Sensor id: 100, Sensor Type: 2000 (LX4000 Pneumo P2)
      2) Sensor id: 101, Sensor Type: 2013 (LX4000 Thoracic Pneumo Line Length)
      3) Sensor id: 102, Sensor Type: 2001 (LX4000 Pneumo P1)
      4) Sensor id: 103, Sensor Type: 2012 (LX4000 Abdominal Pneumo Line Length)
      5) Sensor id: 104, Sensor Type: 2002 (LX4000 GSR)
      6) Sensor id: 105, Sensor Type: 2007 (LX4000 GSR Detrended) - Virtual Sensor
      7) Sensor id: 106, Sensor Type: 2003 (LX4000 Cardio)
      8) Sensor id: 107, Sensor Type: 2004 (LX4000 AUX1)
      9) Sensor id: 108, Sensor Type: 2005 (LX4000 AUX2)
      10) Sensor id: 109, Sensor Type: 2006 (LX4000 AUX3)

LXSoftware version:           11.1.4
Recording start time:         miércoles, 05 de diciembre de 2012 05:48:47 p.m.
Recording end time:           miércoles, 05 de diciembre de 2012 06:00:21 p.m.
Recording time:               11 minutes 34.413000 seconds (694 total seconds)
Total recorded packets:       83340, Num packets expected: 83330, difference -10
Largest interpacket time:     156 milliseconds occurred at: 3.135000 seconds - packet #: 376
Smallest interpacket time:    15 milliseconds occurred at: 8 minutes 44.615000 seconds - packet #: 62960
Average interpacket time:     8.331753 milliseconds
Expected interpacket time:    8.333333 milliseconds
Bytes read: 1166739.0, bytes expected: 1166613.8, diff: 125.2 (8 raw A/D values) 0.074500 seconds
