

***** DAS Statistics *****

   * Id: 0
   * Type: 4 LX-4000 DAS
   * Version: 6
   * Data Rate: 120
   * Sample Size: 4
   * Number of Sensors: 10
      1) Sensor id: 100, Sensor Type: 2000 (LX4000 Pneumo P2)
      2) Sensor id: 101, Sensor Type: 2013 (LX4000 Thoracic Pneumo Line Length)
      3) Sensor id: 102, Sensor Type: 2001 (LX4000 Pneumo P1)
      4) Sensor id: 103, Sensor Type: 2012 (LX4000 Abdominal Pneumo Line Length)
      5) Sensor id: 104, Sensor Type: 2002 (LX4000 GSR)
      6) Sensor id: 105, Sensor Type: 2007 (LX4000 GSR Detrended) - Virtual Sensor
      7) Sensor id: 106, Sensor Type: 2003 (LX4000 Cardio)
      8) Sensor id: 107, Sensor Type: 2004 (LX4000 AUX1)
      9) Sensor id: 108, Sensor Type: 2005 (LX4000 AUX2)
      10) Sensor id: 109, Sensor Type: 2006 (LX4000 AUX3)

Recording start time:         miércoles, 05 de diciembre de 2012 05:21:14 p.m.
Recording end time:           miércoles, 05 de diciembre de 2012 05:33:31 p.m.
Recording time:               12 minutes 17.242000 seconds (737 total seconds)
Total recorded packets:       88485, Num packets expected: 88469, difference -16
Largest interpacket time:     156 milliseconds occurred at: 1.388000 seconds - packet #: 166
Smallest interpacket time:    93 milliseconds occurred at: 1.856000 seconds - packet #: 226
Average interpacket time:     8.331608 milliseconds
Expected interpacket time:    8.333333 milliseconds
Bytes read: 1238836.0, bytes expected: 1238566.6, diff: 269.4 (19 raw A/D values) 0.160381 seconds
